YAESU FT-891 SETUP FOR CW ON CanAm Net

SETUP FOR  AUTO CW mode from SSB on VFO

1: Long press “F” key to get into MENU mode.  
2: Set menu 07-06 CW AUTO MODE to ON
3: Set menu 07-07 CW BFO to AUTO
4: Short press “F” key to exit MENU mode
5: Short press “F” key repeatedly until CW SETTING menu is displayed. 
6: Rotate the MULTI switch until the pointer is beside BK-IN
7: Press the MULTI switch to turn BK-IN to the ON position 
8: Short press the A, B or C button to exit the CW SETTING menu

TO PERFORM A CW QSO on the CanAm net:

1: Use your key to send CW.  When you are finished, the radio will return to LSB.