ALL OTHER RADIOS NOT IN THE LIST

1: Ensure radio is on VFO-A.  If not, press A/B button until VFO-A is displayed. 
2: Dial up 7153 LSB
3: Press A/B button quickly to change to VFO-B and dial up 7152.3 CW mode, VOX turned ON
4: Press A/B button to return to VFO-A

TO PERFORM A CW QSO on CanAm Net:

1: From VFO-A, enable SPLIT operation.
2: VOX should be on and you now make your CW QSO
3: After your CW QSO, disable SPLIT operation to return to SSB mode.  

ALTERNATIVE METHOD

1:   Dial up 7153 LSB on VFO-A
2:   Dial up 7152.3 CW on VFO-B
3:   Switch to VFO-B to make a CW contact
4:   Switch back to VFO-A when done