KENWOOD TS-590S AND TS-590SG SETUP FOR CW ON CanAm Net

STORE MEMORY CHANNEL for SPLIT OPERATION 

1: Ensure radio is on VFO-A.  If not, press A/B button until VFO-A is displayed. 
2: Dial up 7153 LSB
3: Press and hold A/B button for 2 seconds
4: Press A/B button quickly to change to VFO-B and dial up 7152.3 CW mode, VOX turned ON
5: Press A/B button to return to VFO-A
To store this setup in memory: 
6: Press M.IN button, M.CH will display.  Select a blank memory channel with the MULTI/CH switch.  
7: Press M.IN again to store the memory

RECALL MEMORY FOR NET OPERATION

1: Press M/V button once.  Rotate MULTI/CH switch to select the CanAm Net memory channel  
2: Press M>V button once. 
3: Press the SPLIT button so that the display shows 7153 LSB.  

TO PERFORM A CW QSO on CanAm Net:

1: Press SPLIT     Display shows LSB 7153 SPLIT 7152.3
2:  VOX should be on and you now make your CW QSO
3: After your CW QSO, press SPLIT to return to SSB mode.